1. Flash the Qt bootloader for the Cortex M0+ core, see https://doc.qt.io/QtForMCUs/qtul-flashinginstructions-infineon-bootloader.html for instructions
    - TVII-C-2D-4M (CYT3DL): tviic2d4m-baremetal_bootloader.elf
    - TVII-C-2D-6M (CYT4DN): tviic2d6m-baremetal_bootloader.elf
   

2. Flash the Qt GUI application for the Cortex M7 core, see https://doc.qt.io/QtForMCUs/qtul-flashinginstructions-infineon.html
   Note that it's not necessary to set the QUL_DIR variable to flash custom binaries.
    - TVII-C-2D-4M (CYT3DL): tviic2d4m-cluster.elf
    - TVII-C-2D-6M (CYT4DN): tviic2d6m-cluster.elf
